**Important Future Task**

1. It needs to figure out how the simulation time step and control step (time duration from acquiring control input, processing, and applying the control output) can be set up separately. The simulation time step should be less than the control time step.

\*\*The hardware experiment will provide a more clear picture of this issue.